Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package avrora.sim.mcu

Interface Summary
ATMega128L.ADCInput | The `ADCInput` interface is used by inputs into the analog to digital converter.
ATMega128L.Clock | Interface for an alternate clock.
ATMega128L.SPIDevice | Interface for devices that can connect to the SPI.
ATMega128L.USARTDevice | The `USARTDevice` interface describes USARTs and other serial devices which can be connected to the USART.
Microcontroller | The `Microcontroller` interface corresponds to a hardware device that implements the AVR instruction set.
Microcontroller.Pin | The `Pin` interface encapsulates the notion of a physical pin on the microcontroller chip.
Microcontroller.Pin.Input | The `Input` interface represents an input pin.
Microcontroller.Pin.Output | The `Output` interface represents an output pin.
MicrocontrollerFactory | The `MicrocontrollerFactory` interface is implemented by a class that is capable of making repeated copies of a particular microcontroller for use in simulation.
MicrocontrollerProperties | The `MicrocontrollerProperties` interface represents a set of methods that get information about a particular microcontroller implementation.

Class Summary
ATMega128L | The `ATMega128L` class represents the `Microcontroller` instance that has all the hardware parameters of the ATMega128L microcontroller as produced by Atmel Corporatation.
ATMega128L.SPIDevice.SPIFrame | A single byte data frame for the SPI.
ATMega128L.USARTDevice.USARTFrame | A `USARTFrame` is a representation of the serial frames being passed between the USART and a connected device.
Microcontrollers | The `Microcontrollers` class represents a static, known mapping between names and implementations of microcontroller models.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES