Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## avrora.sim.mcu
Class ATMega128L.SimImpl.SPI.TransmitReceive

    java.lang.Object
      avrora.sim.mcu.ATMega128L.SimImpl.SPI.TransmitReceive

All Implemented Interfaces:
  Simulator.Event

Enclosing class:
  ATMega128L.SimImpl.SPI

protected class ATMega128L.SimImpl.SPI.TransmitReceive
extends java.lang.Object
implements Simulator.Event

The SPI transfer event.

Constructor Summary
`protected` | `ATMega128L.SimImpl.SPI.TransmitReceive()`

Method Summary
`protected void` | `enableTransfer()`
`void` | `fire()` Notes.

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Constructor Detail

### ATMega128L.SimImpl.SPI.TransmitReceive

    protected ATMega128L.SimImpl.SPI.TransmitReceive()

Method Detail

### enableTransfer

    protected void enableTransfer()

### fire

    public void fire()

  Notes. The way this delay is setup right now, when the ATMega128L is in master mode and transmits, the connected device has a delayed receive. For the radio, this is not a problem, as the radio is the master and is responsible for ensuring correct delivery time for the SPI.

  Specified by:
    `fire` in interface `Simulator.Event`

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD