Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## avrora.sim.platform
Class ExternalFlash.PD2Input

    java.lang.Object
      avrora.sim.mcu.Microcontroller.InputPin
          avrora.sim.platform.ExternalFlash.PD2Input

All Implemented Interfaces:
  Microcontroller.Pin.Input

Enclosing class:
  ExternalFlash

protected class ExternalFlash.PD2Input
extends Microcontroller.InputPin

Constructor Summary
`protected` | `ExternalFlash.PD2Input()`

Method Summary
`boolean` | `read()` The `read()` method is called by the simulator when the program attempts to read the level of the pin.

Methods inherited from class avrora.sim.mcu.Microcontroller.InputPin
`disableInput, enableInput`

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Constructor Detail

### ExternalFlash.PD2Input

    protected ExternalFlash.PD2Input()

Method Detail

### read

    public boolean read()

  Description copied from interface: `Microcontroller.Pin.Input`
  The `read()` method is called by the simulator when the program attempts to read the level of the pin. The device can then compute and return the current level of the pin.

  Returns:
    true if the level of the pin is high; false otherwise

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD