Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## avrora.sim.radio
Class CC1000Radio.SerialConfigurationInterface.PDATAInput

    java.lang.Object
      avrora.sim.mcu.Microcontroller.InputPin
          avrora.sim.radio.CC1000Radio.SerialConfigurationInterface.PDATAInput

All Implemented Interfaces:
  Microcontroller.Pin.Input

Enclosing class:
  CC1000Radio.SerialConfigurationInterface

protected class CC1000Radio.SerialConfigurationInterface.PDATAInput
extends Microcontroller.InputPin

Constructor Summary
`protected` | `CC1000Radio.SerialConfigurationInterface.PDATAInput()`

Method Summary
`boolean` | `read()` The `read()` method is called by the simulator when the program attempts to read the level of the pin.

Methods inherited from class avrora.sim.mcu.Microcontroller.InputPin
`disableInput, enableInput`

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Constructor Detail

### CC1000Radio.SerialConfigurationInterface.PDATAInput

    protected CC1000Radio.SerialConfigurationInterface.PDATAInput()

Method Detail

### read

    public boolean read()

  Description copied from interface: `Microcontroller.Pin.Input`
  The `read()` method is called by the simulator when the program attempts to read the level of the pin. The device can then compute and return the current level of the pin.

  Returns:
    true if the level of the pin is high; false otherwise

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD