Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## avrora.sim.platform
Class ExternalFlash.PD5Output

    java.lang.Object
      avrora.sim.mcu.Microcontroller.OutputPin
          avrora.sim.platform.ExternalFlash.PD5Output

All Implemented Interfaces:
  Microcontroller.Pin.Output

Enclosing class:
  ExternalFlash

protected class ExternalFlash.PD5Output
extends Microcontroller.OutputPin

Constructor Summary
`protected` | `ExternalFlash.PD5Output()`

Method Summary
`void` | `write(boolean level)` The `write()` method is called by the simulator when the program writes a logical level to the pin.

Methods inherited from class avrora.sim.mcu.Microcontroller.OutputPin
`disableOutput, enableOutput`

Methods inherited from class java.lang.Object
`clone, equals, finalize, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

Constructor Detail

### ExternalFlash.PD5Output

    protected ExternalFlash.PD5Output()

Method Detail

### write

    public void write(boolean level)

  Description copied from interface: `Microcontroller.Pin.Output`
  The `write()` method is called by the simulator when the program writes a logical level to the pin. The device can then take the appropriate action.

  Parameters:
    `level` - a boolean representing the logical level of the write

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD