Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## avrora.sim
Interface InterruptTable.Notification

All Known Implementing Classes:
  ADC.ControlRegister, ATMegaFamily.FlagBit, SPI

Enclosing interface:
  InterruptTable

public static interface InterruptTable.Notification

The `Notification` interface serves a very specific role in simulation; for device implementations to be notified when an interrupt that a device may have posted is executed, or when the user forces an interrupt to be notified. Some interrupts are "auto-clear" which means that they automatically unpost themselves when their handler is invoked. To support this functionality, a `Notification` is inserted on them that allows the flag register to be updated when the handler is invoked. As a user of the simulation, you SHOULD NOT implement a notification.

See Also:
  `for probing interrupts`

Method Summary
`void` | `force(int inum)`
`void` | `invoke(int inum)`

Method Detail

### force

    public void force(int inum)

### invoke

    public void invoke(int inum)

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD